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TECHNICAL REQUIREMENTS FOR ON-BOARD EQUIPMENT

1. Technical requirements for on-board equipment:

	Parameter
	Requirement

	GNSS horizontal accuracy
	≤5 m

	Geolocation data collection interval
	5 s

	Geolocation data transmission interval
	60 s

	Data format
	JSON/XML

	Communication technology
	OBE must use only those mobile communication technologies that are available on the 4G/5G networks of the Republic of Lithuania. 



2. On-board equipment must be authorised for use in Lithuania in accordance with the the Rules on the Approval of On-Board Equipment by Road Toll Service Users;
3. On-board equipment must bear the CE mark and the WEEE (Waste Electrical and Electronic Equipment) marking.
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